,Model##other##,Description##other##,Volts##other##,Cycle##other##,Phase##other##,FL Amps##other##,HP##other##,Conn Plug##other##,Conn Conduit##other##,Depth##other##,Width##other##,Mechanical Remarks##other##,Weight in Pounds##other##
Configuration,,,,,,,,,,,,,
,,,,,,,,,,,,,
SLIM LINE/HALF SOLID DOOR,,,,,,,,,,,,,
SELF-CONTAINED,,,,,,,,,,,,,
,,,,,,,,,,,,,
"1FSENHD (SS Front, Alum. Box)",1FSENHD,"Freezer, Reach-In",120,60,1,7.6,0.5,NEMA 5-15P,0,"35.375""","17.75""",,190
"1FSENSAHD (SS Ext, Alum. Int.)",1FSENSAHD,"Freezer, Reach-In",120,60,1,7.6,0.5,NEMA 5-15P,0,"35.375""","17.75""",,190
"1FSENSSHD (SS Ext, SS Int.)",1FSENSSHD,"Freezer, Reach-In",120,60,1,7.6,0.5,NEMA 5-15P,0,"35.375""","17.75""",,250
,,,,,,,,,,,,,
Options,,,,,,,,,,,,,
Legs or Casters,,,,,,,,,,,,,
Legs (Casters=0),,,,,,,,,,,,,
Casters (Casters=1),,,,,,,,,,,,,
Door Swings,,,,,,,,,,,,,
Left swing (Right Door Hinge=0),,,,,,,,,,,,,
Right swing (Right Door Hinge=1),,,,,,,,,,,,,
