,Model##other##,Description##other##,Volts##other##,Cycle##other##,Phase##other##,FL Amps##other##,HP##other##,Height##other##,Electric Connection Type##other##,Mechanical Remarks##other##,Weight in Pounds##other##
Configuration,,,,,,,,,,,
,,,,,,,,,,,
STANDARD WIDTH/FULL SOLID DOOR,,,,,,,,,,,
SELF-CONTAINED,,,,,,,,,,,
,,,,,,,,,,,
"DL2FI (SS Front, Alum.)",DL2FI ,"Freezer, Roll-In",208,60,1,13.5,1,"86""",115/208V NEUTRAL REQUIRED; 3-WIRE + GROUND,,540
DL2FI-SA (SS Ext. Alum. Int.),DL2FI-SA ,"Freezer, Roll-In",208,60,1,13.5,1,"86""",115/208V NEUTRAL REQUIRED; 3-WIRE + GROUND,,540
DL2FI-SS (SS Ext. SS Int.),DL2FI-SS ,"Freezer, Roll-In",208,60,1,13.5,1,"86""",115/208V NEUTRAL REQUIRED; 3-WIRE + GROUND,,540
,,,,,,,,,,,
EXTENDED HEIGHT/FULL SOLID DOOR,,,,,,,,,,,
SELF-CONTAINED,,,,,,,,,,,
,,,,,,,,,,,
"DL2FI-E  (SS Front, Alum. Box)",DL2FI-E,"Freezer, Roll-In",208,60,1,13.5,1,"92""",115/208V NEUTRAL REQUIRED; 3-WIRE + GROUND,,540
"DL2FI-SA-E (SS Ext, Alum. Int.)",DL2FI-SA-E,"Freezer, Roll-In",208,60,1,13.5,1,"92""",115/208V NEUTRAL REQUIRED; 3-WIRE + GROUND,,540
"DL2FI-SS-E (SS Ext, SS Int.)",DL2FI-SS-E,"Freezer, Roll-In",208,60,1,13.5,1,"92""",115/208V NEUTRAL REQUIRED; 3-WIRE + GROUND,,540
,,,,,,,,,,,
,,,,,,,,,,,
Options,,,,,,,,,,,
Door swing,,,,,,,,,,,
Left swing (Right Door Hinge=0),,,,,,,,,,,
Right swing (Right Door Hinge=1),,,,,,,,,,,
