,Model##other##,Description##other##,Volts##other##,Cycle##other##,Phase##other##,FL Amps##other##,HP##other##,Height##other##,Electric Connection Type##other##,Mechanical Remarks##other##,Weight in Pounds##other##
Configuration,,,,,,,,,,,
,,,,,,,,,,,
STANDARD WIDTH/FULL SOLID DOOR,,,,,,,,,,,
SELF-CONTAINED,,,,,,,,,,,
,,,,,,,,,,,
"DL1FI (SS Front, Alum.)",DL1FI ,"Freezer, Roll-In",208,60,1,10.9,0.75,"86""",120/208V NEUTRAL REQUIRED; 4-WIRE + GROUND,,350
DL1FI-SA (SS Ext. Alum. Int.),DL1FI-SA ,"Freezer, Roll-In",208,60,1,10.9,0.75,"86""",120/208V NEUTRAL REQUIRED; 4-WIRE + GROUND,,350
DL1FI-SS (SS Ext. SS Int.),DL1FI-SS ,"Freezer, Roll-In",208,60,1,10.9,0.75,"86""",120/208V NEUTRAL REQUIRED; 4-WIRE + GROUND,,350
,,,,,,,,,,,
EXTENDED HEIGHT/FULL SOLID DOOR,,,,,,,,,,,
SELF-CONTAINED,,,,,,,,,,,
,,,,,,,,,,,
"DL1FI-E  (SS Front, Alum. Box)",DL1FI-E,"Freezer, Roll-In",208,60,1,10.9,0.75,"92""",120/208V NEUTRAL REQUIRED; 4-WIRE + GROUND,,350
"DL1FI-SA-E (SS Ext, Alum. Int.)",DL1FI-SA-E,"Freezer, Roll-In",208,60,1,10.9,0.75,"92""",120/208V NEUTRAL REQUIRED; 4-WIRE + GROUND,,350
"DL1FI-SS-E (SS Ext, SS Int.)",DL1FI-SS-E,"Freezer, Roll-In",208,60,1,10.9,0.75,"92""",120/208V NEUTRAL REQUIRED; 4-WIRE + GROUND,,350
,,,,,,,,,,,
Options,,,,,,,,,,,
Door swing,,,,,,,,,,,
Left swing (Right Door Hinge=0),,,,,,,,,,,
Right swing (Right Door Hinge=1),,,,,,,,,,,
