,Model##other##,Description##other##,Volts##other##,Cycle##other##,Phase##other##,FL Amps##other##,HP##other##,Conn Plug##other##,Conn Conduit##other##,Depth##other##,Width##other##,Mechanical Remarks##other##,Weight in Pounds##other##
Configuration,,,,,,,,,,,,,
,,,,,,,,,,,,,
SLIM LINE/HALF SOLID DOOR,,,,,,,,,,,,,
SELF-CONTAINED,,,,,,,,,,,,,
,,,,,,,,,,,,,
"2FSENHD (SS Front, Alum. Box)",2FSENHD,"Freezer, Reach-In",120,60,1,8.6,0.5,NEMA 5-15P,0,"35.375""","36.25""",,190
"2FSENSAHD (SS Ext, Alum. Int.)",2FSENSAHD,"Freezer, Reach-In",120,60,1,8.6,0.5,NEMA 5-15P,0,"35.375""","36.25""",,190
"2FSENSSHD (SS Ext, SS Int.)",2FSENSSHD,"Freezer, Reach-In",120,60,1,8.6,0.5,NEMA 5-15P,0,"35.375""","36.25""",,250
,,,,,,,,,,,,,
SLIM LINE/SHALLOW HALF,,,,,,,,,,,,,
SOLID DOOR/ SELF-CONTAINED,,,,,,,,,,,,,
,,,,,,,,,,,,,
"2FSESNHD  (SS Front, Alum. Box)",2FSESNHD,"Freezer, Reach-In",120,60,1,8.6,0.5,NEMA 5-15P,0,"29.25""","36.25""",,190
"2FSESNSAHD (SS Ext, Alum. Int.)",2FSESNSAHD,"Freezer, Reach-In",120,60,1,8.6,0.5,NEMA 5-15P,0,"29.25""","36.25""",,190
"2FSESNSSHD (SS Ext, SS Int.)",2FSESNSSHD,"Freezer, Reach-In",120,60,1,8.6,0.5,NEMA 5-15P,0,"29.25""","36.25""",,250
,,,,,,,,,,,,,
Options,,,,,,,,,,,,,
Legs or Casters,,,,,,,,,,,,,
Legs (Casters=0),,,,,,,,,,,,,
Casters (Casters=1),,,,,,,,,,,,,
Door Swings,,,,,,,,,,,,,
Left Door Left Hinge (Left Door Right Hinge=0),,,,,,,,,,,,,
Left Door Right Hinge (Left Door Right Hinge=1),,,,,,,,,,,,,
Right Door Right Hinge(Right Door Left Hinge =0),,,,,,,,,,,,,
Right Door Right Hinge(Right Door Left Hinge =1),,,,,,,,,,,,,
