, Model##other##, Volts##other##, Cycle##other##, Phase##other##, FL Amps##other##, Weight in Pounds##other##, Code##other##, Description##other##
Configuration,,,,,,,,
,,,,,,,,
ELECTRICAL CONFIGURATION,,,,,,,,
,,,,,,,,
Three Phase,,,,,,,,
,,,,,,,,
3FQE60U_208/60/3,3FQE60U_CM,208,60,3,48,255,1,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_240/60/3,3FQE60U_CM,240,60,3,41,255,1,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_480/60/3,3FQE60U_CM,480,60,3,21,255,1,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_220/60/3,3FQE60U_CM,220,60,3,26,255,1,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_380/60/3,3FQE60U_CM,380,60,3,26,255,1,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_230/60/3,3FQE60U_CM,230,60,3,25,255,1,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_400/60/3,3FQE60U_CM,400,60,3,25,255,1,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_208/60/3*,3FQE60U_DT,208,60,3,48,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_240/60/3*,3FQE60U_DT,240,60,3,41,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_480/60/3*,3FQE60U_DT,480,60,3,21,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_220/60/3*,3FQE60U_DT,220,60,3,26,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_380/60/3*,3FQE60U_DT,380,60,3,26,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_230/60/3*,3FQE60U_DT,230,60,3,25,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_400/60/3*,3FQE60U_DT,400,60,3,25,255,2,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_208/60/3**,3FQE60U_LC,208,60,3,48,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_240/60/3**,3FQE60U_LC,240,60,3,41,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_480/60/3**,3FQE60U_LC,480,60,3,21,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_220/60/3**,3FQE60U_LC,220,60,3,26,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_380/60/3**,3FQE60U_LC,380,60,3,26,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_230/60/3**,3FQE60U_LC,230,60,3,25,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_400/60/3**,3FQE60U_LC,400,60,3,25,255,3,HIGH  PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER


3FQE60U_240/60/3***,3FQE60U_CM,240,60,3,24,255,1,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_240/60/3****,3FQE60U_DT,240,60,3,24,255,2,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_240/60/3*****,3FQE60U_LC,240,60,3,24,255,3,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER
3FQE60U_415/60/3,3FQE60U_CM,415,60,3,24,255,1,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS CM3.5
3FQE60U_415/60/3*,3FQE60U_DT,415,60,3,24,255,2,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS DIGITAL TIMER
3FQE60U_415/60/3**,3FQE60U_LC,415,60,3,24,255,3,HIGH PRODUCTION OIL-CONSERVING ELECTRIC FRYERS LANE CONTROLLER