,Width##LENGTH##INCHES,Weight in Pounds##OTHER##,Watts##ELECTRICAL_WATTAGE##WATTS,W_TopSec##LENGTH##INCHES,Volts##ELECTRICAL_POTENTIAL##VOLTS,URL Cutsheet##OTHER##,Type Mark##OTHER##,Status##OTHER##,Specification by User##OTHER##,Specification by Manufacturer##OTHER##,Show Clearances##OTHER##,Serial Number##OTHER##,Seismic Rating##OTHER##,SMACNA No##OTHER##,Revision Code##OTHER##,Phase##OTHER##,Omniclass Number and Title##OTHER##,Number of Poles##OTHER##,NAFEM Spec ID Number##OTHER##,Model##OTHER##,Min Ckt Ampacity##ELECTRICAL_CURRENT##AMPERES,Max Overcurrent Protection##ELECTRICAL_CURRENT##AMPERES,Masterspec##OTHER##,Manufacturer##OTHER##,KCLRef##OTHER##,KCL SpecSheet URL##OTHER##,Item Number##OTHER##,Installed By##OTHER##,Identify Quantity as Lot##OTHER##,Height##LENGTH##INCHES,HP##OTHER##,Furnished By##OTHER##,Foodservice Equipment Identifier##OTHER##,FL Amps##ELECTRICAL_CURRENT##AMPERES,Electrical Remarks##OTHER##,Elec Conn RI Height##LENGTH##INCHES,Elec Conn Connection Height##LENGTH##INCHES,Description##OTHER##,Depth_Bowel_Cnt##LENGTH##INCHES,Cycle##ELECTRICAL_FREQUENCY##HERTZ,Conn Plug##OTHER##,Conn Conduit##OTHER##,CSI MasterFormat##OTHER##,Bowel_Rad##LENGTH##INCHES,Base##LENGTH##INCHES,Assembly Code##OTHER##,Apparent Power##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES
QF_Univex_SL250RB,34.253680133722,2264,18409.599999999999,27.166000000000,220.000000000000,,,,,,1,,,,,3,,1,,SL250RB,0.000000000000,0.000000000000,,Univex,,,,,1,58.304106590321,31,,1,83.680000000000,,0.000000000000,0.000000000000,Spiral Mixer,43.060000000000,60.000000000000,,0,11 40 00,13.937000000000,0.000000000000,E1090300,31848.608000000000
